**CLPe Series**

**Manual Programming Cheat Sheet**

1. **Turn the radio OFF**
2. **Enter programming mode by doing the following (must have earpiece connected)**
   1. Press and hold the **PTT**, **VOLUME +**, and **POWER** buttons.
   2. Keep all three buttons held down until you hear a chirping pattern with a “programming mode” voice prompt. The LED should be blinking GREEN or BLUE.
3. **Adjust your settings**
   1. Tap the **MENU** button once, and you will hear a channel number. Press **VOLUME UP** or **VOLUME DOWN** button to select your desired channel, once on your desired channel, proceed to below steps:
      1. Tap the **MENU** button once, and you will hear a “Frequency” number. Change to the desired number by pressing the **VOLUME UP** or **VOLUME DOWN** button.
      2. Tap the **MENU** button once, and you will a “Code” number. Change to the desired number by pressing the **VOLUME UP** or **VOLUME DOWN** button.
      3. IF you need to change the settings on additional channels, tap the **MENU** button again until you hear the “Channel” number prompt and repeat the steps above. If you are finished, proceed to the next step to save your settings.
4. **Save settings and exit programming mode**
   1. To save settings and exit programming mode, press and hold the **PTT** button until the radio beeps. The LED will go back to the normal color according to radio channel (Red for Ch 1).

**A picture containing black, dark

Description automatically generated![A picture containing text, tableware, clipart, plate

Description automatically generated]()**

**MENU**

**POWER**

**VOLUME UP / VOLUME DOWN**

**PTT**

**LED RING**